{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":85,"n_cols":4,"rows_kept":85,"merged":[[0,0,0,3],[84,0,84,3]]}
["汕头职业技术学院院本部和金园校区校舍补漏项目估算工程量"]
["序号","项目名称","数量","单位"]
["一","外墙裂缝渗水入室内"]
[1,"实验楼第一计算室",6,"m"]
[null,"实验楼第9计算室",10,"m"]
[null,"第二实验楼607A室",10,"m"]
[null,"B栋宿舍C1010房",10,"m"]
[null,"合计外墙修补",36,"m"]
["①","顺裂缝用切割机切V型槽并清理干净",36,"m"]
["②","填补PT0035伸缩防水胶",36,"m"]
["③","钉10目锌网",36,"m"]
["④","批刮水泥沙(加防水剂)",36,"m"]
["⑤","贴墙面砖",36,"m"]
[2,"外墙体外墙专用透明胶"]
[null,"第一实验楼第一计算室东西外墙",25,"㎡"]
[null,"第一实验楼第九计算室南面及西面角",25,"㎡"]
[null,"B栋宿舍101房外墙",25,"㎡"]
[null,"合计",75,"㎡"]
["①","JS万可涂外墙砖用胶二遍",75,"㎡"]
[3,"混泥土天花板裂缝渗漏灌浆"]
[null,"第一实验楼第一计算室天面栏墙边",5,"m"]
[null,"第一实验楼第八计算室",5,"m"]
[null,"教学楼314办公室天花板",8,"m"]
[null,"第二食堂1楼天花板  ",25,"m"]
[null,"B栋宿舍A5010房天花板",5,"m"]
[null,"B栋宿舍C1010房天花板 ",8,"m"]
[null,"合计",56,"m"]
["①","专用灌浆钉",56,"m"]
["②","灌浆液(水溶性聚氨脂注浆液)",56,"m"]
["③","打孔锁钉",56,"m"]
["④","灌浆",56,"m"]
["⑤","拆钉头堵孔",56,"m"]
["⑥","清洗剂",56,"m"]
[4,"因渗漏室内批灰、油漆霉烂等修复"]
[null,"第一实验楼第一计算室",12,"㎡"]
[null,"第一实验楼第三计算室(3.8m×0.9m)+(4.5m×0.9m)=7.47㎡",10,"㎡"]
[null,"第一实验楼第九计算室",15,"㎡"]
[null,"教学楼314办公室",10,"㎡"]
[null,"第二实验楼607A",8,"㎡"]
[null,"第二教学楼2区A301房",8,"㎡"]
[null,"B栋宿舍A5010房",6,"㎡"]
[null,"B栋宿舍C1010房",6,"㎡"]
[null,"B栋宿舍A6010房 ",2]
[null,"合计",77,"㎡"]
["①","铲除霉烂批灰",77,"㎡"]
["②","批刮腻子粉",77,"㎡"]
["③","打磨刷乳胶漆",77,"㎡"]
["④","室内地面地毯防护",5,"处"]
[5,"五号楼铁皮房漏水修复"]
["①","凿除铁皮与墙交接处填补胶泥及老化填缝胶",35,"m"]
["②","在铁皮与墙交接处用切割机切缝并清理干净",35,"m"]
["③","用0.5厘彩铁板插入缝内紧贴原铁皮瓦面并加装柳钉紧固",35,"m"]
["④","填补PP5硅酮结构密封胶",35,"m"]
[6,"教学楼伸缩缝不锈板与墙交接缝处理"]
[null,"第一实验楼第三计算室外墙窗框边交接缝",35,"m"]
["①","清除清除老化填缝胶",35,"m"]
["②","填补995硅酮结构密封胶",35,"m"]
[7,"第一实验楼第一计算室上方天面做过墙排水管1处"]
["①","凿墙穿洞工费",1,"项"]
["②","Φ75PVC管0.5m安装封口",1,"项"]
[8,"教学搂2区A401房天面排水管周边漏水处理"]
["①","凿排水管周边混泥土板5公分深并清理干净",1,"项"]
["②","填补PT0035确保时防水材料",1,"项"]
["③","刷德安密K11防水胶",1,"项"]
[null,"第三教学楼顶层天面围栏漏水。外墙空鼓破裂"]
["二","天面围栏与板面相交处裂缝漏水处理"]
[1,"凿除围栏与板面交接处八字水泥块并清理干净",90,"m"]
[2,"铺贴伸缩防水卷材成L型",90,"m"]
[3,"辅料丙稀酸黏合剂",90,"m"]
[4,"表面填补水泥沙厚3公分压光",90,"m"]
["三","围栏外墙因漏水空鼓破裂修补",60,"m"]
[1,"用切割机对空鼓范围切开与牢固砖体隔开",60,"m"]
[2,"凿除空鼓贴砖及批灰",60,"m"]
[3,"在凿除部位刷固沙剂",60,"m"]
[4,"钉10目镀锌铁网",60,"m"]
[5,"刮灰（水泥沙1：2）",60,"m"]
[6,"调与墙体砖相仿颜色漆压面",60,"m"]
["四","卫生间等清通"]
[1,"幼师1.2楼厕所卫生间3个"]
[2,"教学1号大楼4、5楼卫生间6个、地漏2个"]
[null,"合计清通",11,"个"]
["五","幼师1楼地下排污管清通"]
["①","幼师1楼地下排污地面开挖掏树根清通",1,"处"]
["②","混凝土复原、地砖复原(30×30)",1,"项"]
["注：实际工程量以届时竣工验收实测工程量为准。"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}